Set-up procedures to connect to the Roadkill – troubleshooting the connection

1. To have the manual ribbon cable link, connect first to the computer, then to the roadkill. Be sure that the red wire is on the side of the green screw box.
2. To run code:
   1. Tools>Programmer>AVSIPR mrkII (serial)
   2. Tools>Board>Arbotix
   3. Tools>Serial Port>COM(high number)
   4. Verify
   5. File>Upload using programmer

Noted Challenges:

* Can talk to the board in one direction, communication is not active though
* The Serial Monitor was not responding to input, nor reading from the Arbotix